**Randwick Village Hall Dishwasher Instructions v3 23/1/23**

1. Power on machine at wall switch.
2. Open door and check drain plug is in place.

A picture containing indoor

Description automatically generated

1. Close door and press start button

A picture containing text, indoor, oven, stove

Description automatically generated

When this button is first pressed the machine operates through a sequence of filling the tank with water and heating it up. **This may take 30minutes.** The rinse temperature must

be min 85degC and tank temp min 55degC.

A picture containing text, indoor, steel, stainless

Description automatically generated

1. Once at temperature load the machine.

A picture containing indoor, dish rack, metal, kitchen appliance

Description automatically generated

**Cutlery**

**Pans**

**Crockery**

**Note**: this is not a waste disposal unit and any solid waste should be rinsed off in the sink before loaded in the washer.

5. Close the door and select your wash time by using one of the three buttons on the right side of the control panel. They require a short press to activate the wash cycle.

Button 1 Short wash (90s)

Button 2 Medium length wash (120s)

Button 3 Long wash (180s)

A picture containing indoor, person, oven

Description automatically generated

**180s**

**120s**

**90s**

1. When the wash cycle is complete open the door, unload and reload and restart the cycle (step 5).
2. Once you have finished with the dishwasher open the front door and remove the plug ready for the drain down cycle.

A picture containing indoor, person, oven

Description automatically generated

1. **With the door open** hold button 1 down for **4 seconds,** the button will flash, and the water will drain away slowly.

A picture containing indoor, person, oven

Description automatically generated

1. Once empty rinse out the bottom of the machine with a jug of fresh water.

A picture containing text, person, indoor, oven

Description automatically generated

10. After it has drained remove the filter and rinse solids down sink.

A picture containing person, indoor

Description automatically generated

1. Replace the filter and drain plug and power off.



1. Leave the door open to dry the machine out.

**Switch off at the wall after use!**